Skip to content

# Class Member Variables

## a

- api_version (bluespy_audio_codec_lib_info)
- AGC (bluespy_capture_audiopod_options)
- audiopod_opts (bluespy_capture_options)
- audio_channel_allocation (bluespy_cis_lc3_config)

## b

- bias (bluespy_capture_audiopod_options)
- bits_per_ch (bluespy_capture_i2s_options)
- b (bluespy_query_value)
- bluespy_query_value (bluespy_query_value)
- bytes (bluespy_query_value)

## c

- channel_index (bluespy_audio_channel_t)
- config (bluespy_audio_codec_info)
- config_len (bluespy_audio_codec_info)
- container (bluespy_audio_codec_info)
- context_handle (bluespy_audio_codec_init_ret)
- codec_name (bluespy_audio_codec_lib_info)
- count (bluespy_audiopod_current_data, bluespy_custom_decoder_status_t, bluespy_spectrum_data)
- channels (bluespy_capture_audiopod_options)
- current_probe (bluespy_capture_audiopod_options)
- codec_frames_per_SDU (bluespy_cis_lc3_config)
- children (bluespy_custom_event)
- change_mask (bluespy_logic_change)

## d

- decode (bluespy_audio_codec_funcs)
- deinit (bluespy_audio_codec_funcs)
- data (bluespy_audiopod_current_data, bluespy_audiostream_id_span, bluespy_bytes, bluespy_connection_id_span, bluespy_spectrum_data)
- DRC (bluespy_capture_audiopod_options)
- DSP_mode (bluespy_capture_i2s_options)
- disable_AGC (bluespy_capture_options)
- disable_HDT_dewhitening (bluespy_capture_options)
- description (bluespy_custom_query)
- d (bluespy_query_value)

## e

- error (bluespy_audio_codec_init_ret)
- enable_15_4 (bluespy_capture_options)
- enable_CL (bluespy_capture_options, bluespy_multi_moreph_options)
- enable_Channel_Sounding (bluespy_capture_options)
- enable_Dukosi (bluespy_capture_options)
- enable_HDT (bluespy_capture_options)
- enable_LE (bluespy_capture_options, bluespy_multi_moreph_options)
- enable_MHDT_CL (bluespy_capture_options)
- enable_MHDT_LE (bluespy_capture_options)
- enable_Proprietary_1 (bluespy_capture_options)
- enable_Proprietary_2 (bluespy_capture_options)
- enable_QHS (bluespy_capture_options)
- enable_Varjo (bluespy_capture_options)
- enable_wifi (bluespy_capture_options, bluespy_multi_moreph_options)
- enabled (bluespy_custom_decoder_status_t)

## f

- fns (bluespy_audio_codec_init_ret)
- format (bluespy_audio_codec_init_ret)
- first_chan_follows_WS_high (bluespy_capture_i2s_options)
- frame_duration_us (bluespy_cis_lc3_config)

## i

- ID (bluespy_audio_channel_t)
- input (bluespy_capture_audiopod_options)
- i2s_opts (bluespy_capture_options)
- i (bluespy_query_value)
- id (bluespy_query_value)
- interval (bluespy_spectrum_data)

## k

- keep_i2s_and_audiopod (bluespy_filter_file_options)
- keep_logic (bluespy_filter_file_options)
- keep_spectrum (bluespy_filter_file_options)
- keep_uart (bluespy_filter_file_options)
- key (bluespy_key)

## l

- len (bluespy_bytes)
- LA_high_voltage (bluespy_capture_audiopod_options)
- LA_low_voltage (bluespy_capture_audiopod_options)
- logic_mask (bluespy_capture_options)
- logic_rate (bluespy_capture_options)
- logic_use_external_vref (bluespy_capture_options)
- layer (bluespy_custom_event)
- length (bluespy_key)

## m

- MSB_first (bluespy_capture_i2s_options)
- master (bluespy_capture_i2s_options)
- mask_payloads (bluespy_capture_options)
- maximum_input_signal_dbm (bluespy_capture_options)
- multi_moreph_opts (bluespy_capture_options)
- measurement_time (bluespy_latency_result)

## n

- n_channels (bluespy_audio_codec_decoded_format, bluespy_capture_i2s_options)
- names (bluespy_custom_decoder_status_t)
- n_children (bluespy_custom_event)

## o

- output (bluespy_capture_audiopod_options)
- one_sample_delay (bluespy_capture_i2s_options)
- octets_per_codec_frame (bluespy_cis_lc3_config)

## p

- power_supply_V (bluespy_capture_audiopod_options)
- presentation_delay_us (bluespy_cis_lc3_config)
- pretty_name (bluespy_custom_query)
- peak_ratio (bluespy_latency_result)

## q

- query (bluespy_custom_event, bluespy_custom_query)

## r

- range_start (bluespy_filter_file_options)

## s

- sample_format (bluespy_audio_codec_decoded_format)
- sample_rate (bluespy_audio_codec_decoded_format, bluespy_capture_audiopod_options)
- size (bluespy_audiostream_id_span, bluespy_connection_id_span)
- second_I2S_input (bluespy_capture_audiopod_options)
- SCLK_line (bluespy_capture_i2s_options)
- SD_line (bluespy_capture_i2s_options)
- sample_on_rising_edge (bluespy_capture_i2s_options)
- spectrum_period (bluespy_capture_options)
- sampling_frequency_Hz (bluespy_cis_lc3_config)
- status (bluespy_latency_result)
- state (bluespy_logic_change)
- s (bluespy_query_value)

## t

- three_measurements_expected (bluespy_latency_result)
- time_difference_max_ns (bluespy_latency_result)
- time_difference_min_ns (bluespy_latency_result)
- time_difference_ns (bluespy_latency_result)
- total_energy (bluespy_latency_result)
- time (bluespy_logic_change)
- type (bluespy_query_value)

## v

- VIO_dV (bluespy_capture_audiopod_options)
- vol_in_left (bluespy_capture_audiopod_options)
- vol_in_right (bluespy_capture_audiopod_options)
- vol_out_left (bluespy_capture_audiopod_options)
- vol_out_right (bluespy_capture_audiopod_options)

## w

- WS_line (bluespy_capture_i2s_options)