Skip to content

# Struct bluespy_capture_audiopod_options

ClassList > bluespy_capture_audiopod_options

## Public Attributes

Type | Name
--- | ---
bool | AGC
bool | DRC
double | LA_high_voltage
double | LA_low_voltage
double | VIO_dV
bluespy_audio_bias | bias
bluespy_audio_channel | channels
bool | current_probe
bluespy_audio_connect | input
bluespy_audio_connect | output
double | power_supply_V
uint32_t | sample_rate
bool | second_I2S_input
double | vol_in_left
double | vol_in_right
double | vol_out_left
double | vol_out_right

## Public Attributes Documentation

### variable AGC

    bool bluespy_capture_audiopod_options::AGC;

### variable DRC

    bool bluespy_capture_audiopod_options::DRC;

### variable LA_high_voltage

    double bluespy_capture_audiopod_options::LA_high_voltage;

### variable LA_low_voltage

    double bluespy_capture_audiopod_options::LA_low_voltage;

LA_low_voltage and LA_high_voltage must be within the range of 0.0 to 3.3

### variable VIO_dV

    double bluespy_capture_audiopod_options::VIO_dV;

### variable bias

    bluespy_audio_bias bluespy_capture_audiopod_options::bias;

### variable channels

    bluespy_audio_channel bluespy_capture_audiopod_options::channels;

### variable current_probe

    bool bluespy_capture_audiopod_options::current_probe;

### variable input

    bluespy_audio_connect bluespy_capture_audiopod_options::input;

### variable output

    bluespy_audio_connect bluespy_capture_audiopod_options::output;

### variable power_supply_V

    double bluespy_capture_audiopod_options::power_supply_V;

power_supply_V must be within the range of 0.6 to 5.0

### variable sample_rate

    uint32_t bluespy_capture_audiopod_options::sample_rate;

Valid sample rates in Hz are: 8'000, 11'025, 16'000, 22'050, 32'000, 44'100, 48'000, 88'200, 96'000, 176'400, 192'000

### variable second_I2S_input

    bool bluespy_capture_audiopod_options::second_I2S_input;

### variable vol_in_left

    double bluespy_capture_audiopod_options::vol_in_left;

### variable vol_in_right

    double bluespy_capture_audiopod_options::vol_in_right;

### variable vol_out_left

    double bluespy_capture_audiopod_options::vol_out_left;

### variable vol_out_right

    double bluespy_capture_audiopod_options::vol_out_right;

The documentation for this class was generated from the following file `bluespy.h`