Skip to content

# Struct bluespy_capture_options

ClassList > bluespy_capture_options

## Public Attributes

Type | Name
--- | ---
bluespy_capture_audiopod_options * | audiopod_opts
bool | disable_AGC
bool | disable_HDT_dewhitening
bool | enable_15_4
bool | enable_CL
bool | enable_Channel_Sounding
bool | enable_Dukosi
bool | enable_HDT
bool | enable_LE
bool | enable_MHDT_CL
bool | enable_MHDT_LE
bool | enable_Proprietary_1
bool | enable_Proprietary_2
bool | enable_QHS
bool | enable_Varjo
bool | enable_wifi
bluespy_capture_i2s_options * | i2s_opts
uint32_t | logic_mask
bluespy_logic_rate | logic_rate
bool | logic_use_external_vref
bool | mask_payloads
int16_t | maximum_input_signal_dbm
bluespy_multi_moreph_options | multi_moreph_opts
uint16_t | spectrum_period

## Public Attributes Documentation

### variable audiopod_opts

    bluespy_capture_audiopod_options* bluespy_capture_options::audiopod_opts;

### variable disable_AGC

    bool bluespy_capture_options::disable_AGC;

### variable disable_HDT_dewhitening

    bool bluespy_capture_options::disable_HDT_dewhitening;

### variable enable_15_4

    bool bluespy_capture_options::enable_15_4;

### variable enable_CL

    bool bluespy_capture_options::enable_CL;

### variable enable_Channel_Sounding

    bool bluespy_capture_options::enable_Channel_Sounding;

### variable enable_Dukosi

    bool bluespy_capture_options::enable_Dukosi;

### variable enable_HDT

    bool bluespy_capture_options::enable_HDT;

### variable enable_LE

    bool bluespy_capture_options::enable_LE;

### variable enable_MHDT_CL

    bool bluespy_capture_options::enable_MHDT_CL;

### variable enable_MHDT_LE

    bool bluespy_capture_options::enable_MHDT_LE;

### variable enable_Proprietary_1

    bool bluespy_capture_options::enable_Proprietary_1;

### variable enable_Proprietary_2

    bool bluespy_capture_options::enable_Proprietary_2;

### variable enable_QHS

    bool bluespy_capture_options::enable_QHS;

### variable enable_Varjo

    bool bluespy_capture_options::enable_Varjo;

### variable enable_wifi

    bool bluespy_capture_options::enable_wifi;

### variable i2s_opts

    bluespy_capture_i2s_options* bluespy_capture_options::i2s_opts[2];

### variable logic_mask

    uint32_t bluespy_capture_options::logic_mask;

### variable logic_rate

    bluespy_logic_rate bluespy_capture_options::logic_rate;

### variable logic_use_external_vref

    bool bluespy_capture_options::logic_use_external_vref;

### variable mask_payloads

    bool bluespy_capture_options::mask_payloads;

### variable maximum_input_signal_dbm

    int16_t bluespy_capture_options::maximum_input_signal_dbm;

### variable multi_moreph_opts

    bluespy_multi_moreph_options bluespy_capture_options::multi_moreph_opts[32];

If multiple Morephs are connected, capture options specific to each device after the first (LE, CL, WiFi).

### variable spectrum_period

    uint16_t bluespy_capture_options::spectrum_period;

Valid spectrum periods in microseconds are: 5, 10, 20, 50, 100, 200, 500, 1000, 2000, 5000, 10000

0 to disable spectrum capture.

The documentation for this class was generated from the following file `bluespy.h`